Ergogen <version> CLI

Interpreting format: YAML
Preprocessing input...
Calculating variables...
Parsing points...
Generating outlines...
Modeling cases...
Scaffolding PCBs...
Output would be empty, rerunning in debug mode...
Writing output to disk...
Done.

